For 1990-2009 cars

#### Special Tools

• | EN 46106 Engine Flywheel Holding Tool

• | J 45059 Angle Meter

1. Place the engine flywheel in position on the crankshaft.
2. Install 2 NEW bolts in location at the top and bottom of the engine flywheel bolt pattern allowing the engine flywheel to hang in position.
3. Install the EN 46106 .

Caution: Refer to Fastener Caution in the Preface section.

4. Install the remaining NEW engine flywheel bolts.

Tighten

1. Tighten the NEW engine flywheel bolts to 30 N·m (22 lb ft).
2. Tighten the NEW engine flywheel bolts an additional 45 degrees using the J 45059 .