For 1990-2009 cars

### Removal Procedure

1. Remove the driver side instrument panel (I/P) insulator closeout panel. Refer to Instrument Panel Insulator Replacement - Left Side .
2. Remove the bolt (1) securing the brake pedal position switch to the brake panel bracket.
3. Remove the switch.

### Installation Procedure

1. Connect the electrical connector on the switch.
2. Align the brake panel position switch to the stud (3).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the bolt (1) securing the brake panel position switch to the brake panel bracket.

Tighten
Tighten the bolt (1) to 9 N·m (80 lb in).

4. Install the driver side instrument panel (I/P) insulator closeout panel. Refer to Instrument Panel Insulator Replacement - Left Side .
5. Recalibrate the brake pedal position (BPP) sensor. Refer to Brake Pedal Position Sensor Calibration .