For 1990-2009 cars

### Removal Procedure

1. Remove the driver side instrument panel (I/P) closeout/insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side or Instrument Panel Insulator Replacement - Left Side .
2. Remove the flasher module (2) off the I/P carrier.
3. Disconnect the electrical connector (1).

### Installation Procedure

1. Connect the electrical connector (1) to the flasher module (2).
2. Slide the flasher module retaining clip onto the I/P carrier.
3. Install the driver side instrument panel (I/P) closeout/insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side or Instrument Panel Insulator Replacement - Left Side .