For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Important: Hold the shaft link stud with a hex tool to prevent damage to the link seal.

2. Remove the stabilizer shaft link to the stabilizer shaft upper retaining nuts.
3. Remove the stabilizer shaft link to lower control arm lower retaining nut.
4. Remove the stabilizer shaft link from the vehicle.

### Installation Procedure

1. Install the stabilizer shaft link to the vehicle.

Important: Do not tighten the nuts at this time.

Important: Hold the shaft link stud with a hex tool to prevent damage to the link seal.

2. Install the stabilizer shaft link lower retaining nut.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the stabilizer shaft link upper retaining nut.
4. Install the stabilizer shaft link upper and lower retaining nut.

Tighten

• | Tighten the nuts to 114 N·m (84 lb ft).

• | Tighten the nuts to 125 N·m(103 lb ft)

5. Lower the vehicle.