For 1990-2009 cars

### Left Camshaft Cover

1. Remove and discard the camshaft cover bolt grommets.
2. Remove the fuel injector sight shield ballstud.
3. Remove the oil fill cap.

Important: Do not reuse the camshaft cover gasket and spark plug shield tube seals.

4. Remove and discard the left camshaft cover gasket.
5. Remove and discard the left spark plug shield tube seals.

### Right Camshaft Cover

1. Remove and discard the right camshaft cover bolt grommets.

Important: Do not reuse the camshaft cover gasket and spark plug shield tube seals.

2. Remove and discard the right camshaft cover gasket.
3. Remove and discard the right spark plug shield tube seals.