For 1990-2009 cars

Notice: Refer to Fastener Notice in the Preface section.

1. Install the oil pressure sender.

Tighten
Tighten the oil pressure sender to 20 N·m (15 lb in).

2. Install the NEW oil filter cartridge.
3. If the oil filter cap O-ring is removed, install a NEW O-ring on the oil filter cap.

3.1. | Ensure the O-ring groove is not damaged. Replace the oil filter cap if the O-ring groove is damaged.

3.2. | Protect the O-ring from damage during installation by covering the threads of the oil filter cap with tape or plastic wrap.

3.3. | DO NOT stretch the O-ring during installation.

3.4. | Roll the O-ring into position over the covered threads.

3.5. | Remove the tape or plastic wrap from the oil filter cap threads.

3.6. | Ensure the oil filter cap threads are clean.

4. Lubricate the oil filter cap threads and O-ring with clean engine oil.
5. Install the oil filter cap.

Tighten
Tighten the oil filter cap to 25 N·m (18 lb in).