For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Rear Side Door Trim Panel Replacement .
2. Disconnect the electrical connectors.
3. Release the tabs securing the switch the door trim panel.
4. Remove the switch through the bottom of the door trim panel.

### Installation Procedure

1. Push the switch into the door trim panel in order to secure the mounting tabs.
2. Connect the electrical connectors.
3. Install the door trim panel. Refer to Rear Side Door Trim Panel Replacement .