For 1990-2009 cars

### Removal Procedure

1. Open the engine hood.
2. Remove the front grille.
3. Disconnect the electrical connector.
4. Remove the horn retaining bolts to remove the horn.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Fix the horn to the body rail.

Tighten
Tighten the horn bolt to 9 N·m (80 lb in).

2. Connect the horn electrical connectors.
3. Install the front grille.
4. Close the hood.