For 1990-2009 cars

### Removal Procedure

Caution: In order to prevent damage to the paint, mask the roof panel in front of the sunroof opening using masking tape and paper.

1. Cycle the sunroof window to the vent position.
2. Slide the sunshade rearward.
3. Disconnect the sunroof panel side opening closeout covers (5) from the retention clips (1,3,4) in order to access the sunroof window screws (2,6).
4. Tape the sunroof panel side opening closeout covers in a downward position.
5. Remove the sunroof window screws (1) on both sides.

Note: Be careful not to scratch the roof surface or the sunroof window.

6. Lift the sunroof window (3) from the sunroof opening.

### Installation Procedure

1. Position the sunroof window (3) into the opening, with the window trade mark pointing rearward.
2. Install the sunroof window screws (1).
3. Finger tighten the screws, do not tighten.
4. Carefully close the sunroof window from the vent position to the full closed position.
5. Adjust the sunroof window. Refer to Sunroof Window Height and Opening Fit Adjustment.
6. Connect the sunroof panel side opening closeout covers (2) to the sunroof window clips.
7. Snap the sunroof panel side opening closeout covers into the sunroof window retention clips.
8. Close the sunshade.
9. Cycle the sunroof window to ensure proper operation and fit.