For 1990-2009 cars

#### Special Tools

J 38778 Door Trim Pad Clip Remover

### Removal Procedure

1. Remove the rear seat cushion. Refer to Rear Seat Cushion replacement (Luxury) .
2. Using a J 38778 release the retainer clips from the rocker panel.
3. Remove the rear carpet retainer.

### Installation Procedure

1. Position the rear carpet retainer with the slots in the rocker.
2. Press downward in order to engage the retainers into the slots in the rocker panel.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement (Luxury) .