For 1990-2009 cars

### Removal Procedure

1. Remove the rear compartment trim panel. Refer to Rear Compartment Sill Trim Plate Replacement .
2. Remove the bolts securing the amplifier to the vehicle.
3. Disconnect the electrical connector.
4. Remove the amplifier.

### Installation Procedure

1. Connect the electrical connectors.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the amplifier to the vehicle.

Tighten
Tighten the bolts (1) to 9 N·m (80 lb in).

3. Install the rear compartment trim. Refer to Rear Compartment Sill Trim Plate Replacement .