For 1990-2009 cars

### Diagnostic Instructions

• | Perform the Diagnostic System Check - Vehicle prior to using this diagnostic procedure.

• | Review Strategy Based Diagnosis for an overview of the diagnostic approach.

• | Diagnostic Procedure Instructions provides an overview of each diagnostic category.

### DTC Descriptors

DTC P0667: Transmission Control Module (TCM) Temperature Sensor Performance
DTC P0668: Transmission Control Module (TCM) Temperature Sensor Circuit Low Voltage
DTC P0669: Transmission Control Module (TCM) Temperature Sensor Circuit High Voltage

### Circuit/System Description

The transmission control module (TCM) temperature sensor is located inside of the control solenoid (w/body and TCM) valve assembly and is not serviced separately. The TCM temperature sensor provides the temperature of the TCM. This temperature reading is used in various shifting and diagnostic routines in the TCM software. This fault is handled inside the TCM and no external circuits are involved.

### Conditions for Running the DTC

#### P0667

• | DTCs P0667, P0711, P0712, P0713, P0716, P0717, P0722 and P0723 are not set.

• | Start the ignition voltage, run the engine.

• | The TCM temperature is between -54 and +149°C (-65 and +300°F).

#### P0668

• | Start the ignition voltage, run the engine.

• | DTC P0668 passed this ignition cycle.

#### P0669

• | Start the ignition voltage, run the engine.

• | DTC P0669, P0716, P0717, P0722, P0723 are not set.

• | The transmission output shaft speed is greater than 200 RPM for greater than 200 seconds.

• | The TCC slip speed is equal to or greater than 120 RPM for 200 seconds.

### Conditions for Setting the DTC

#### P0667

• | Fail Case 1

- | Vehicle speed is greater than 8 km/h (5 mph) for 300 seconds cumulative.

- | Torque converter clutch (TCC) slip speed is greater than 120 RPM for 300 seconds cumulative.

- | The TCM temperature is between -55 and +21°C (-67 and +70°F).

- | The TCM temperature has changed by less than 2.0°C (3.6°F) in 100 seconds.

- | The transmission fluid temperature (TFT) is greater than 70°C (158°F).

- | The TFT has increased by 55°C (99°F) since startup.

• | Fail Case 2

- | Vehicle speed is greater than 8 km/h (5 mph) for 300 seconds cumulative.

- | TCC slip speed is greater than 120 RPM for 300 seconds cumulative.

- | The TCM temperature is between 120-150°C (248-302°F).

- | The TCM temperature has changed by less than 2.0°C (3.6°F) in 100 seconds.

- | The TFT is greater than 70°C (158°F).

- | The TFT has increased by 55°C (99°F) since startup.

• | Fail Case 3

| The TCM temperature changes by greater than or equal to 20°C (36°F) 14 times over 7 seconds.

#### P0668

The TCM temperature is greater than or equal to 249°C (480°F) for greater than 4 seconds.

#### P0669

The TCM temperature is less than or equal to -249°C (-316°F) for greater than 10 seconds.

### Action Taken When the DTC Sets

• | DTCs P0667, P0668, and P0669 are Type C DTCs.

• | The TCM allows the vehicle to operate in transmission protection mode.

### Conditions for Clearing the DTC

DTCs P0667, P0668, and P0669 are Type C DTCs.

### Diagnostic Aids

Reprogram the TCM and retest the DTC to see if the DTC resets. Perform the Control Solenoid Valve and Transmission Control Module Assembly Inspection before replacing the control solenoid (w/body and TCM) valve assembly.

### Reference Information

#### Schematic Reference

Automatic Transmission Controls Schematics

#### Connector End View Reference

• | Automatic Transmission Inline 16-Way Connector End View

• | Automatic Transmission Internal Connector End Views

• | Automatic Transmission Related Connector End Views

#### DTC Type Reference

• | Diagnostic Trouble Code (DTC) Type Definitions

• | Diagnostic Trouble Code (DTC) List/Type

#### Electrical Information Reference

• | Circuit Testing

• | Connector Repairs

• | Testing for Intermittent Conditions and Poor Connections

• | Wiring Repairs

### Circuit/System Verification

#### P0667

1. Start the engine and operate the vehicle at 64 km/h (40 mph) while observing the TCM power up temperature sensor and the TCM temperature sensor.
2. The system is operating normally if the TCM power up temperature is within 10°C (18°F) of the TCM temperature sensor.

#### P0668 and P0669

Start the engine and check for DTCs P0668 and P0669.

### Circuit/System Testing

1. Clear the DTC and operate the vehicle under the condition for running and setting the DTC.
2. Verify that the DTC does not reset.

⇒ | If the DTC resets, replace the control solenoid (w/body and TCM) valve assembly.

### Component Testing

Perform the Control Solenoid Valve and Transmission Control Module Assembly Inspection .

### Repair Instructions

Perform the Diagnostic Repair Verification after completing the diagnostic procedure.

1. Control solenoid (w/body and TCM) valve assembly replacement. Refer to Control Module References for replacement, setup, and programming.
2. Perform the Service Fast Learn Adapts .