For 1990-2009 cars

### Removal Procedure

1. Remove the I/P cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
2. Disconnect the aspirator hose from the inside air temperature sensor.
3. Disconnect the electrical connectors from the inside air temperature sensor.
4. Remove inside air temperature sensor retaining screws.
5. Remove the inside air temperature sensor.

### Installation Procedure

1. Install the inside air temperature sensor.
2. Install the inside air temperature sensor retaining screws.
3. Connect the electrical connector to the inside air temperature sensor.
4. Connect the aspirator hose to the inside air temperature sensor.
5. Install the I/P cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.