For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission fluid pan and filter. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .

1 | Manual Shift Shaft Position Switch Assembly Electrical Connector Tip

• | Release the connector lock before disconnecting. Engage the connector lock after connecting.

• | The wiring harness clip near the connector does not need to be replaced if broken or missing. The clip is used during manufacturing to keep the wire harness clear during an automated bolt installation process. If the clip is damaged, simply remove and discard.

2 | Notice: Refer to Fastener Notice in the Preface section. Manual Shift Shaft Position Switch Assembly Bolt Tighten 8 N·m (71 lb in)
3 | Manual Shift Shaft Position Switch Assembly Tip

• | Align the switch activator slide with the manual valve link.

• | It is recommended that transmission adaptive pressure (TAP) information be reset. Resetting the TAP values using a scan tool will erase all learned values in all cells. As a result, the engine control module (ECM), powertrain control module (PCM) or transmission control module (TCM) will need to relearn TAP values. Transmission performance may be affected as new TAP values are learned. Reset the TAP values. Refer to Transmission Adaptive Functions .