For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.
2. Remove the bolts securing the instrument cluster.
3. Disconnect the electrical connector and remove the instrument cluster.

### Installation Procedure

1. Disconnect the electrical connector and install the instrument cluster.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the bolts securing the instrument cluster.

Tighten
Tighten the bolts to 2 N·m (9 lb in).

3. Install the instrument cluster trim panel. Refer to Instrument Cluster Trim Panel Replacement.