For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Ref No.* | Qty | Size | Specification
--- | --- | --- | --- | ---
Metric | English
Accumulator Housing to Valve Body | 318 | 12 | M6x1.0x30.0 | 11 N·m | 97 lb in
Channel Plate to Valve Body | 300 | 7 | M6x1.0x38.0 | 11 N·m | 97 lb in
Converter Housing to Case | 2 | 7 | M8x1.25x35.0 | 22 N·m | 16 lb ft
Detent Spring Bolt | -- | -- | -- | 11 N·m | 97 lb in
Drain Plug to Fluid Pan | 63 | 1 | M14x1.5x10.0 | 20 N·m | 15 lb ft
Drive Flange Nut | -- | -- | -- | 57 N·m | 42 lb ft
Extension Housing to Case | 35 | 7 | M8x1.25x35.0 | 22 N·m | 16 lb ft
Fluid Fill Plug | -- | -- | -- | 20 N·m | 15 lb ft
Fluid Pan to Case | 65 | 20 | M6x1.0x16.0 | 11 N·m | 97 lb in
Front Control Valve Body to Top Channel Plate | 50 | 2 | M6x1.0x38.0 | 11 N·m | 97 lb in
Input Speed Sensor to Case | 45 | 1 | M6x1.0x20.0 | 11 N·m | 97 lb in
Manual Shift Shaft Nut | -- | -- | -- | 16 N·m | 11 lb ft
Oil Pressure Test Plug | -- | -- | -- | 11 N·m | 97 lb in
Output Speed Sensor to Case | 43 | 1 | M6x1.0x30.0 | 11 N·m | 97 lb in
Parking Pawl Actuator Bracket to Case | 609 | 2 | M8x1.25x25.0 | 22 N·m | 16 lb ft
Prop Shaft Flange to Output Shaft | 34 | 1 | M22x1.5x10.0 | 57 N·m | 42 lb ft
Shift Control Assembly to Tunnel Reinforcement Nut | -- | -- | -- | 12 N·m | 106 lb in
Shift Control Linkage Adjustment Nut | -- | -- | -- | 6 N·m | 53 lb in
Torque Converter Bolt | -- | -- | -- | 63 N·m | 46 lb ft
Torque Converter Housing Seal Bolt | 228 | 2 | M4x0.7x10.0 | 3.6 N·m | 31.86 lb in
Transmission Fluid Pump Cover to Torque Converter Housing | 240 | 6 | M6x1.0x40.0 | 11 N·m | 97 lb in
Transmission Fluid Pump Cover to Torque Converter Housing | 241 | 5 | M8x1.25x40.0 | 22 N·m | 16 lb ft
Transmission Fluid Level Hole Plug to Case | 36 | 1 | M18x1.5x12.0 | 20 N·m | 15 lb ft
Transmission Mount Bracket to Body Bolt | -- | -- | -- | 58 N·m | 43 lb ft
Transmission Mount Bracket to Transmission - 5L40-E | -- | -- | -- | 63 N·m | 46 lb ft
Transmission Mounting Bolt M10x1.5 | -- | -- | -- | 50 N·m | 37 lb ft
Transmission Mounting Bolt M12x1.75 | -- | -- | -- | 75 N·m | 55 lb ft
Transmission Oil Cooler Line to Cooling Fan Shroud Bolts | -- | -- | -- | 6.5 N·m | 58 lb in
Transmission Oil Cooler Line to Transmission Oil Cooler Fittings | -- | -- | -- | 20 N·m | 15 lb ft
Transmission Oil Cooler Line to Transmission Retainer Bolt | -- | -- | -- | 25 N·m | 18 lb ft
Transmission Oil Cooler Mounting Bolts | -- | -- | -- | 5 N·m | 44 lb in
Transmission Oil Cooler Retainer Bracket Bolt | -- | -- | -- | 25 N·m | 18 lb ft
Transmission Pressure Test Plug to Case | 40 | 1 | M10x1.0x8.0 | 11 N·m | 97 lb in
Valve Body to Case | 49 | 2 | M6x1.0x50.0 | 11 N·m | 97 lb in
Valve Body to Case | 51 | 6 | M6x1.0x50.0 | 11 N·m | 97 lb in
Valve Body to Case | 53 | 1 | M6x1.0x68.0 | 11 N·m | 97 lb in
Valve Body to Channel Plate | 53 | 1 | M6x1.0x68.0 | 11 N·m | 97 lb in
* Reference number refers to the callout number in the disassembled view.