For 1990-2009 cars

### Removal Procedure

Warning: Refer to Exhaust Service Warning in the Preface section.

Warning: Refer to Protective Goggles and Glove Warning in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Apply a suitable lubricant to the following in order to ease the removal of the hangers (2).

• | The left exhaust hanger mounting bracket rod (1)

• | The tail pipe hanger rods (3)

3. Pry the tail pipe hangers (2) free from the tail pipe hanger rods (3).
4. Pry the tail pipe hangers (2) free from the exhaust hanger mounting bracket rods (1).
5. Remove the nuts securing the rear energy absorber and the exhaust hanger mounting bracket (2) to the rear compartment rail.
6. Remove the exhaust hangers mounting bracket from the rear energy absorber.

### Installation Procedure

1. Position the exhaust hangers mounting bracket (2) between the rear energy absorber and the stud plate (1).

Insert the stud plate (1) through the exhaust hangers mounting bracket (2), the rear energy absorber and the rear compartment rail.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the nuts securing the rear energy absorber and the exhaust hangers mounting bracket (2) to the rear compartment rail.

Tighten
Tighten the bumper nuts to 25 N·m (18 lb ft).

3. Apply a soapy solution to the following in order to ease the installation of the hangers:

• | The left exhaust hanger mounting bracket rod (1)

• | The inner diameter of the tail pipe hangers (2)

• | The tail pipe hanger rods (3)

4. Press the tail pipe hangers (2) over the tail pipe hanger rods (3).
5. Press the tail pipe hangers (2) over the exhaust hangers mounting bracket rods (1).
6. Lower the vehicle.