For 1990-2009 cars

### Removal Procedure

1. Remove the headliner. Refer to Headlining Trim Panel Replacement.
2. Remove the sunroof control console.
3. Disconnect the electrical connectors from the sunroof motor and control module.
4. Cut the electrical harness to the harness clip.
5. Remove the rear compartment trim panel. Refer to Rear Compartment Sill Trim Plate Replacement.
6. Disconnect the electrical harness retainer from the rear sunroof drain hose.

Caution: Note the correct routing of the electrical wiring. Failure to reinstall the wiring properly could result in damage to the wiring.

7. Disconnect the electrical connector (1) from the main electrical harness (2).
8. Be careful to pull out the harness through the shoulder belt retractor from the vehicle.
9. Remove the electrical harness from the vehicle.

### Installation Procedure

1. Install the single end connector behind the shoulder retractor to the rear compartment.
2. Connect the electrical connector (1) to the main electrical harness (2).
3. Install the rear compartment trim panel. Refer to Rear Compartment Sill Trim Plate Replacement.
4. Secure the electrical harness clip to the rear drain hose.
5. Connect the electrical connectors to the sunroof motor and control module.
6. Position the electrical connector harness clip to the roof headliner.
7. Verify the operation of the sunroof.
8. Install the headliner. Refer to Headlining Trim Panel Replacement.