For 1990-2009 cars

#### Special Tools

J 29184 Oil Seal Installer

### Removal Procedure

1. Remove the A/C compressor and power steering pump drive belt. Refer to Air Conditioning Compressor and Power Steering Pump Belt Replacement .
2. Remove the generator and water pump drive belt. Refer to Water Pump and Generator Belt Replacement .
3. Remove the crankshaft balancer. Refer to Crankshaft Balancer Removal .
4. Use a flat-bladed tool in order to remove the crankshaft oil seal.

### Installation Procedure

Important: Do not lubricate the crankshaft front oil seal or the crankshaft balancer sealing surfaces.

1. Use the J 29184 or equivalent to install the crankshaft front oil seal.
2. Install the crankshaft balancer. Refer to Crankshaft Balancer Installation .
3. Install the generator and water pump drive belt. Refer to Air Conditioning Compressor and Power Steering Pump Belt Tensioner Replacement .
4. Install the A/C compressor and power steering pump drive belt. Refer to Water Pump and Generator Belt Tensioner Replacement .