For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.
2. Remove the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement .
3. Disconnect the mass air flow (MAF) electrical connector.
4. Remove the air cleaner bolts.
5. Remove the air cleaner.

### Installation Procedure

1. Install the air cleaner.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the air cleaner bolts.

Tighten
Tighten the air cleaner bolts to 9 N·m (78 lb in).

3. Connect the MAF electrical connector.
4. Install the air cleaner intake duct. Refer to Air Cleaner Inlet Duct Replacement .