For 1990-2009 cars

### Removal Procedure

1. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement .
2. Remove the engine front cover. Refer to Engine Front Cover Replacement .
3. Remove the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Removal - Right Side .
4. Remove the right bank secondary camshaft drive chain shoe. Refer to Secondary Camshaft Drive Chain Shoe Removal - Right Side .
5. Remove the right bank secondary camshaft drive chain guide. Refer to Secondary Camshaft Drive Chain Guide Removal - Right Side .
6. Remove the right bank secondary camshaft drive chain. Refer to Secondary Camshaft Drive Chain Removal - Right Side .

### Installation Procedure

1. Install the right bank secondary camshaft drive chain. Refer to Secondary Camshaft Drive Chain Installation - Right Side .
2. Install the right bank secondary camshaft drive chain guide. Refer to Secondary Camshaft Drive Chain Guide Installation - Right Side .
3. Install the right bank secondary camshaft drive chain shoe. Refer to Secondary Camshaft Drive Chain Shoe Installation - Right Side .
4. Install the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Installation - Right Side .
5. Install the spark plugs. Refer to Spark Plug Replacement .
6. Install the engine front cover. Refer to Engine Front Cover Replacement .