For 1990-2009 cars

Table 1: | Low and Reverse Clutch Plate Removal
Table 2: | Low and Reverse Clutch Piston Removal
Table 3: | Low and Reverse Clutch Piston Installation
Table 4: | Low and Reverse Clutch Plate Installation

### Low and Reverse Clutch Plate Removal

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Backing Plate Retaining Ring
2 | Low and Reverse Clutch Backing Plate
3 | Low and Reverse Clutch Plate Assembly (Qty: 6)
4 | Low and Reverse Clutch Plate (Qty: 6)
5 | Low and Reverse Clutch (Waved) Plate

### Low and Reverse Clutch Piston Removal

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Spring Retaining Ring Notice: Ensure the DT-48069 contacts the sprag assembly and not the sprag retaining ring or damage to the sprag may result.

#### Special Tools

DT-48069 Low Clutch Spring Compressor

2 | Low Clutch Sprag Assembly
3 | Low and Reverse Clutch Spring
4 | Low and Reverse Clutch Piston Assembly Tip It may be necessary to apply air to the apply passage in order to unseat the piston.
5 | Low Clutch Sprag Seal Notice: Refer to Seal Reuse Notice in the Preface section.

### Low and Reverse Clutch Piston Installation

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch Piston Assembly Tip Lubricate the inner and outer sealing surfaces of the piston assembly with automatic transmission fluid (ATF) in order to ease installation into the center support assembly.
2 | Low Clutch Sprag Seal Notice: Refer to Seal Reuse Notice in the Preface section. Tip Apply ATF to the DT-48070 to ease seal installation.

#### Special Tools

DT-48070 Low Clutch Sprag Seal Cone

3 | Low and Reverse Clutch Spring Notice: Ensure the spring tabs are facing up during installation. Failure to do so may cause damage to the clutch assembly.
4 | Low Clutch Sprag Assembly Tip

• | Verify that the low clutch sprag is operating correctly. Refer to the illustration for proper freewheel direction.

• | Ensure the missing splines on the sprag assembly are aligned with the missing splines on the center support hub.

5 | Low and Reverse Clutch Spring Retaining Ring Notice: Ensure the DT-48069 contacts the sprag assembly and not the sprag retaining ring or damage to the sprag may result. Notice: The retaining ring gap must be aligned with the 3 missing splines on the center support hub. Failure to do so may cause damage to the clutch assembly.

#### Special Tools

• | DT-48068-1 Low Clutch Sprag Retaining Ring Cone

• | DT-48068-2 Low Clutch Sprag Retaining Ring Pusher

• | DT-48069 Low Clutch Spring Compressor

### Low and Reverse Clutch Plate Installation

Callout | Component Name
--- | ---
1 | Low and Reverse Clutch (Waved) Plate
2 | Low and Reverse Clutch Plate (Qty: 6)
3 | Low and Reverse Clutch Plate Assembly (Qty: 6)
4 | Low and Reverse Clutch Backing Plate
5 | Low and Reverse Clutch Backing Plate Retaining Ring Tip Apply air to verify proper installation of all low and reverse clutch components.