For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Remove the rear seat cushion. Refer to Rear Seat Cushion Replacement.
2. Remove the seat belt buckle fasteners and remove the seat belt buckle.
3. Disconnect the wiring connection to the left and right seat belt buckles.
4. Remove the seat belt buckles from the floor pan.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat belt buckles to the floor pan.

Tighten
Tighten the seat belt buckle fasteners to 42 N·m (31 lb ft).

2. Connect the left and right rear seat belt buckle electrical connectors.
3. Install the rear seat cushion. Refer to Rear Seat Cushion Replacement.