For 1990-2009 cars

Paint Condition | Wet Sanding | Cleaning | Polish
--- | --- | --- | ---
New Vehicle Preparation or Fine Sand Wheel Trace | -- | -- | No Vortex Polishing (M-82) W-6000 Pad, Equipped for DA Polisher
Vortex Trace, Chemical Corrosion or Light Oxidization | -- | -- | No Vortex Polish (M-83) W- 9000 Trim Pad
Over Due Paint or Medium Oxidization | -- | Rough Grinding Cleaner (M- 85) W-7000 Rough Grinding Pad | Vortex Polish (M-82) W-9000 Trim Pad
Heavy oxidation or minor acid rain pitting | -- | Compound Electrical Cleaner (M-84) W-4000 Rough Grinding Pad | No Vortex Polish (M-82) W- 6000 Trim Pad
Dust nibs | 2000 Class Uniform Grain Grinding Stone | Compound Electrical Cleaner (M-84) W-7000 Rough Grinding Pad | No Vortex Polish (M-2) W- 9000 Trim Pad
Minor scratches or acid rain pitting | 2000 Grade Unigrit Sanding Paper | Compound Electrical Cleaner (M-84) W-7000 Rough Grinding Pad | No Vortex Polish (M-2) W- 9000 Trim Pad
Major runs or sags | 1500 Grade Unigrit Sanding Block | Compound Electrical Cleaner (M-84) W-7000 Rough Grinding Pad | No Vortex Polishing (M-2) W- 6000 Pad, Equipped for DA Polisher
Heavy orange peel or acid rain pitting | 1500 Grade Unigrit Sanding Paper | Compound Electrical Cleaner (M-84) W-7000 Rough Grinding Pad | No Vortex Polishing (M-2) W- 6000 Pad, Equipped for DA Polisher
Need protection | -- | -- | Quick Detailer (M-6601) will provide protection without streaking. Contains the mildest of cleaners which will ensure even application of polish.