For 1990-2009 cars

### Removal Procedure

1. Remove the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement .
2. Disconnect the traction control electrical connector.
3. Remove the 2 traction control mounting screws (1).
4. Remove the trim plate.
5. Remove the traction control switch (2).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the traction control switch (2) to the trim plate.
2. Install the two traction control mounting screws (1).

Tighten
Tighten two traction control mounting screws to 2 N·m (18 lb in).

3. Connect the traction control electrical connector.
4. Install the console shift lever bezel. Refer to Console Shift Lever Bezel Replacement .