For 1990-2009 cars

### Removal Procedure

1. Remove the rear floor console. Refer to Rear Floor Console Replacement .
2. Remove the trim panel on both sides of the bridge console.
3. Remove the bolts securing the rear of the bridge console to the bracket.
4. Remove the bolts securing the front of the bridge console to the front floor console.
5. Remove the bridge console.

### Installation Procedure

1. Install the bridge console.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolts securing the front of the bridge console to the front floor console.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

3. Install the bolts securing the rear of the bridge console to the bracket.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

4. Install the trim panels on both sides of the bridge console.
5. Install the rear floor console. Refer to Rear Floor Console Replacement .