For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
The following approximate capacities are given in English and metric conversions. All capacities are approximate. When adding, be sure to fill to the approximate level as recommended in this manual. Recheck fluid level after filling.
Cooling System

- 3.6L (LY7)

11.1 L

11.7 qt

- 4.6L (LH2)

11.9 L

12.6 qt

Engine Oil with Filter

- 3.6L (LY7)

5.7. L

6.0 qt

- 4.6L (LH2)

7.6 L, RWD

8.0 qt, RWD

Fuel Tank | 67 L | 17.7 gal
Transmission/Transmission Drive Axle

- 5L40-E

7.4 L

7.0 qt

- 6L50-E

7.3 L

6.9 qt

Rear Axle | 1.3 L | 1.37 qt