For 1990-2009 cars

Callout | Component Name
--- | ---
Important: The manual shaft must be removed to replace the manual shaft seal.

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission fluid pan. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .
3. Remove the manual shaft detent assembly roller. Refer to Control Valve Lower Body and Upper Body Replacement .

1 | Manual Shaft Detent Lever Hub Pin Important: Discard the pin. Replace with NEW pin. Tip "Walk" the pin out using side cutters.
2 | Manual Shift Shaft Pin Important: Discard the pin. Replace with NEW pin. Tip "Walk" the pin out using side cutters.
3 | Manual Shift Shaft
4 | Manual Shift Shaft Seal Tip

• | Use the J 45201 to remove the seal from the transmission case.

• | Use the J 43909 to install the seal into the transmission case.

#### Special Tools

• | J 45201 Cooler Line Seal Remover

• | J 43909 Selector Shaft Seal Installer