For 1990-2009 cars

### Removal Procedure

1. Remove the left air outlet.
2. Remove the trim panel below the driver information switch on the right side of left air outlet.
3. Remove the bolts retaining the instrument cluster trim panel.
4. Remove the instrument cluster trim panel.
5. Disconnect the electrical connector and the air duct.

### Installation Procedure

1. Connect the electrical connector and the air duct.
2. Install the instrument cluster trim panel.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the bolts retaining the instrument cluster trim panel.

Tighten
Tighten the bolts to 2 N·m (18 lb in).

4. Install the trim panel below the driver information switch on the right side of left air outlet.
5. Install the left air outlet.