For 1990-2009 cars

Table 1: | BCM Scan Tool Data List
Table 2: | DPM Scan Tool Data List
Table 3: | IPC Scan Tool Data List

#### BCM Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Column Lock Relay Command | The body control module | On/Off | On
Column Lock Relay Signal | The body control module | On/Off | On
Battery Voltage Signal | Load Management | Volts | 12.6
Telescope Forward Switch | Inputs | Active/Inactive | Inactive
Telescope Rearward Switch | Inputs | Active/Inactive | Inactive
Tilt Down Switch | Inputs | Active/Inactive | Inactive
Tilt Up Switch | inputs | Active/Inactive | Inactive

#### DPM Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Default Telescope Exit Position | Telescope Sensor | Volts | 3.76V
Default Tilt Exit Position | Tilt Sensor | Volts | 3.76V
Memory Position - Driver 1 | Telescope Sensor | Volts | Varies
Memory Position - Driver 1 | Tilt Sensor | Volts | Varies
Memory Position - Driver 2 | Telescope Sensor | Volts | Varies
Memory Position - Driver 2 | Tilt Sensor | Volts | Varies
Memory 1 Telescope Exit Position | Telescope Sensor | Volts | Varies
Memory 1 Tilt Exit Position | Tilt Sensor | Volts | Varies
Memory 2 Telescope Exit Position | Telescope Sensor | Volts | Varies
Memory 2 Tilt Exit Position | Tilt Sensor | Volts | Varies
Telescope Forward Command | Telescope Sensor | On/Off | Off
Telescope Rearward Command | Telescope Sensor | On/Off | Off
Telescope Sensor | Telescope Sensor | Volt/Counts | 0.7-3.2V (45-37 Counts)
Tilt Down Command | Tilt Sensor | On/Off | Off
Tilt Sensor | Tilt Sensor | Volt/Counts | 1.6-4.2V (88-207 Counts)
Tilt Up Command | Tilt Sensor | On/Off | Off

#### IPC Scan Tool Data List

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Turn the Ignition ON, with the Engine OFF
Battery Voltage Signal | Instrument Panel Cluster (IPC) | Volts | 12.6 V
Column Feedback Signal | Instrument Panel Cluster (IPC) | Volts | 11.9V
Column Lock Enable Signal | Instrument Panel Cluster (IPC) | Enabled/Disabled | Enabled
Column Lock Module Status | Instrument Panel Cluster (IPC) | Enabled/Disabled | Enabled
Column Lock Motor Command | Instrument Panel Cluster (IPC) | Lock/Unlock/Idle/Invalid | Unlock
Column Lock Motor Status | Instrument Panel Cluster (IPC) | Lock/Unlock/Idle/Invalid | Idle
Column Lock Status | Instrument Panel Cluster (IPC) | Varies | Unlocked
Ignition Voltage Signal | Instrument Panel Cluster (IPC) | On/Off | On
Park Switch | Instrument Panel Cluster (IPC) | On/Off | On
Password Status | Instrument Panel Cluster (IPC) | Valid/Invalid/Not Programmed | Valid
Telescope Forward Switch | Instrument Panel Cluster (IPC) | Active/Inactive | Inactive
Telescope Rearward Switch | Instrument Panel Cluster (IPC) | Active/Inactive | Inactive
Tilt Down Switch | Instrument Panel Cluster (IPC) | Active/Inactive | Inactive
Tilt Up Switch | Instrument Panel Cluster (IPC) | Active/Inactive | Inactive