For 1990-2009 cars

### Removal Procedure

1. Remove the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .
2. Remove the sail panel. Refer to Sail Panel Replacement .
3. Remove C-pillar lower trim panel.

### Installation Procedure

1. Install C-pillar lower trim panel.
2. Install the sail panel. Refer to Sail Panel Replacement .
3. Install the rear carpet retainer. Refer to Rear Carpet Retainer Replacement .