For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seat. Refer to Driver or Passenger Seat Replacement .
2. Remove the front seat switch trim panel assembly. Refer to Power Seat Switch Replacement .
3. Remove the front seat trim panel. Refer to Front Seat Trim Panel Replacement .
4. Remove the front seat head restraint and head restraint guide bushes. Refer to Front Seat Head Restraint Replacement .
5. Remove the front seat side airbag. Refer to Driver or Passenger Seat Side Inflatable Restraint Module Replacement .
6. Remove front seat back cover, pad, heater and blower. Refer to Driver or Passenger Seat Back Ventilation Heating and Cooling Blower Replacement .

1 | Front Seat Back Frame Fixed Bolt (Qty: 4) Notice: Refer to Fastener Notice in the Preface section. Tighten 30 N·m (22 lb ft)
2 | Front Seat Back Frame