For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the exhaust system. Refer to Exhaust System Replacement .
3. Remove the drive shaft. Refer to Rear Propeller Shaft Replacement .
4. Support the transmission with a suitable jack.
5. Remove the transmission mount assembly. Refer to Transmission Mount Replacement .
6. Remove the transmission extension housing assembly. Refer to Case Extension and Seal Replacement .

1 | Output Shaft Seal Tip

• | Use the J 45000 to remove the seal. Use care in order to avoid damaging the output shaft bushing.

• | Lubricate the seal with clean transmission fluid.

• | Use the J 38693 to install the seal.

#### Special Tools

• | J 45000 Seal Remover

• | J 38693 Seal Installer