For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

1. Remove the front seats. Refer to Driver or Passenger Seat Replacement .
2. Remove the front seat cushion. Refer to Driver or Passenger Seat Cushion Ventilation Heating and Cooling Blower Replacement .
3. Remove the front seat head and head guide bush. Refer to Front Seat Head Restraint Replacement .
4. Remove the front seat side air bag. Refer to Driver or Passenger Seat Side Inflatable Restraint Module Replacement .
5. Remove the front seat back cover, pad, heater and blower. Refer to Driver or Passenger Seat Cushion Ventilation Heating and Cooling Blower Replacement .

1 | Front Seat Lumbar

#### Procedure:

1. Disconnect the electrical connectors.
2. Pull the lower end of the lumbar forward to disengage the retainers, then slide downward to remove lumbar assembly.