For 1990-2009 cars

### Removal Procedure

1. Remove the left sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.
2. Disconnect the electrical connector from the park brake warning lamp switch.
3. Remove the park brake warning lamp switch retaining bolt.
4. Remove the park brake warning lamp switch.

### Installation Procedure

1. Install the park brake warning lamp switch to the park brake lever assembly. Align the locator pin to the locator hole.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the park brake switch retaining bolt.

Tighten
Tighten the screw to 2 N·m (18 lb ft).

3. Connect the park brake warning lamp electrical connector to the park brake warning lamp switch.
4. Install the left sound insulator panel. Refer to Instrument Panel Insulator Replacement - Left Side.