For 1990-2009 cars

Callout | Component Procedure
--- | ---
1 | Manual Shift Shaft Seal Notice: Do not damage the case bore during removal of the manual shift shaft seal. Notice: When installing the seal, ensure the seal lip is firmly seated against the case bore surface. Do not allow the seal lip to be crushed, or a leak may result.

Notice: Refer to Seal Reuse Notice in the Preface section.

#### Special Tools

• | DT 47770 Seal Installer

• | J 45201 Cooler Line Seal Remover