For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Side Door Sill Nameplate Replacement.
2. Remove the fastening screws of the upper and lower grain garnish from the back of the front door trim panel.
3. Remove the upper and lower grain garnish.

### Installation Procedure

1. Install the upper and lower grain garnish to the front door trim panel.
2. Install fixing screws of the upper and lower grain garnish.
3. Install the front door trim panel. Refer to Side Door Sill Nameplate Replacement.