For 1990-2009 cars

## Headlamp Leveling Switch Replacement Front

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle
2. Remove the right front tire and wheel assembly. Refer to Tire and Wheel Removal and Installation
3. Disconnect the electrical connector (1).
4. Disconnect the ball and socket (1) from the vehicle.
5. Remove the bolt (2) from the sensor.
6. Remove the sensor from the vehicle.

### Installation Procedure

1. Position the sensor to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the bolt (2) to secure the sensor to the vehicle.

Tighten
Tighten the bolt to 9 N.m (80 lb in).

3. Install the ball and socket (1) to the sensor.
4. Connect the electrical connector (1) to the sensor.
5. Install the right tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
6. Lower the vehicle.