For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bridge Console Fastening Bolts | 9 N·m | 80 lb in
Center Support Bracket to I/P Carrier | 10 N·m | 90 lb in
Console Mounting Fasteners | 9 N·m | 80 lb ft
Hood Release Lever Fasteners | 2 N·m | 18 lb in
HVAC Outlet Duct to Carrier | 2 N·m | 18 lb in
I/P Carrier to Cowl | 25 N·m | 18 lb ft
I/P Center Trim to I/P | 2 N·m | 18 lb in
I/P Cluster to I/P | 2 N·m | 18 lb in
I/P Compartment Bin Screws | 2 N·m | 18 lb in
I/P Compartment Door Screws | 2 N·m | 18 lb in
I/P Retainer to Floor Bracket | 10 N·m | 90 lb in
Insulator Panel to I/P | 2 N·m | 18 lb in
Knee Bolster Bracket to I/P | 10 N·m | 90 lb in
Knee Bolster Trim Screws | 2 N·m | 18 lb in
Park Brake Bracket to Carrier | 25 N·m | 18 lb ft
Park Brake Release Lever Fasteners | 2 N·m | 18 lb in
Radio to I/P | 9 N·m | 80 lb in
SIR I/P Module | 12 N·m | 9 lb in
Upper I/P Retainer to Carrier | 10 N·m | 80 lb in