For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the stabilizer shaft mounting bolts.
3. Remove the stabilizer shaft brackets.
4. Remove the stabilizer shaft insulator from the stabilizer shaft.

### Installation Procedure

1. Install the stabilizer shaft insulator to the stabilizer shaft with the slit facing forwards.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the stabilizer shaft bracket.
3. Install the stabilizer shaft bracket mounting bolts.

Tighten
Tighten the bolts to 62 N·m (45 lb ft).

4. Lower the vehicle.