For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement.
2. Remove the bolts securing the knee bolster bracket and remove the bolster bracket.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the knee bolster bracket and the bolts securing the bolster bracket.

Tighten
Tighten the bolts to 9 N·m (80 lb in).

2. Install the knee bolster. Refer to Knee Bolster Replacement.