For 1990-2009 cars

### Removal Procedure

1. Remove the trim plate.
2. Move the sound insulator away from the shock tower.
3. Disconnect the electrical connector (1) on vehicles equipped with F55 suspension.
4. Remove the upper shock mounting nuts (2).
5. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
6. Disconnect the automatic level control from the shock absorber on vehicles with F55 suspension.

Twist the retaining clip and pull the connector from the shock.

7. Remove the lower shock absorber mounting bolt.
8. Remove the shock absorber from the vehicle.

### Installation Procedure

1. Install the shock absorber to the vehicle.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the lower shock absorber mounting bolt.

Tighten
Tighten the bolts to 150 N·m (111 lb ft).

3. Connect the automatic level control air line to the shock.
4. Guide the shock to the body while lowering the vehicle.
5. Install the upper shock mounting nuts (2).

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

6. Connect the electrical connector (1) on vehicles equipped with F55 suspension.
7. Reposition the sound insulator around the shock tower.
8. Install the trim panel.