For 1990-2009 cars

### Removal Procedure

1. Remove the passenger side instrument panel (I/P) insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side .
2. Disconnect the electrical connector (2).
3. Remove the bulb out of I/P insulator panel.

### Installation Procedure

1. Install the bulb to the I/P insulator panel.
2. Connect the electrical connector (2).
3. Install I/P insulator panel. Refer to Instrument Panel Insulator Replacement - Right Side .