For 1990-2009 cars

### Removal Procedure

1. Remove the push-in retainers (1) securing the rear wheelhouse liner to the vehicle.
2. Remove the screws (2) securing the rear wheelhouse liner to the vehicle.
3. Remove the rear wheelhouse liner from the vehicle.

### Installation Procedure

1. Position the rear wheelhouse liner to the vehicle.
2. Install the push-in retainers (1) securing the rear wheelhouse liner to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the screws (2) securing the rear wheelhouse liner to the vehicle.

Tighten
Tighten the bolt to 6 N·m (53 lb in).