For 1990-2009 cars

### Removal Procedure

Note: The area around the electronic brake control module (EBCM) must be free from loose dirt to prevent contamination of disassembled ABS components.

1. Thoroughly clean all contaminants from around the EBCM.
2. Disconnect the brake fluid pressure sensor electrical connector (3) from the brake fluid pressure sensor (2).
3. Remove the brake fluid pressure sensor (2) from the EBCM (1).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the brake fluid pressure sensor (2) to the EBCM (1).

Tighten
Tighten the brake fluid pressure sensor to 17 N·m (13 lb ft).

2. Connect the brake fluid pressure sensor electrical connector (3) to the brake fluid pressure sensor (2).
3. Fill and bleed the hydraulic brake system. Refer to Master Cylinder Reservoir Filling and Hydraulic Brake System Bleeding.
4. Perform the Auto Bleed Procedure. Refer to Antilock Brake System Automated Bleed Procedure.
5. Perform the Diagnostic System Check - Vehicle. Refer to Diagnostic System Check - Vehicle.