For 1990-2009 cars

### Removal Procedure

Caution: Refer to SIR Caution in the Preface section.

1. Disable the SIR system. Refer to SIR Disabling and Enabling Zone 3 .
2. Remove the knee bolster. Refer to Knee Bolster Replacement .
3. Disconnect the electrical connector from the telescope actuator assembly.
4. Remove the fastener bolt (2) from the telescope actuator assembly.
5. Remove the telescope actuator assembly (1) from the steering column.
6. Remove the potentiometer housing (3) from the telescope actuator assembly.
7. Disconnect the telescope cable from the telescope actuator assembly.

### Installation Procedure

1. Install the white end of the telescope actuator cable assembly to the steering column.
2. Install the black end of the telescope actuator cable to the telescope actuator assembly.
3. Install the potentiometer housing (3) to the telescope actuator assembly (1).
4. Install the telescope actuator assembly.

Notice: Refer to Fastener Notice in the Preface section.

5. Install the retaining bolt (2) to the telescope actuator assembly.

Tighten
Tighten the bolts to 5 N·m (44 lb in).

6. Connect the electrical connector to the telescope assembly actuator.
7. Install the knee bolsters. Refer to Knee Bolster Replacement .
8. Enable the SIR system. Refer to SIR Disabling and Enabling Zone 3 .