For 1990-2009 cars

Callout | Component Name
--- | ---

#### Outside Mirror Glass Replacement

6 | Outside Rearview Mirror Glass Caution: Refer to Glass and Sheet Metal Handling Caution in the Preface section.

#### Procedure

1. Apply masking tape to the top of the outside of the mirror housing to prevent damage.
2. Push the mirror face inward at the bottom until full travel is reached.
3. Insert a J 38778 or equivalent behind the glass and the first rib support and pry outward until the mirror face is released.
4. When installing the mirror glass align the mirror face to the backing plate and apply pressure, using a rubber sanding block or equivalent, until an audible click is heard.

#### Special Tools

J 38778 Door Trim Pad Clip Remover