For 1990-2009 cars

### Removal Procedure

1. Apply 2 layers of masking tape on the windshield next to the reveal molding being serviced.
2. Starting from the top, use a plastic flat-bladed tool to pry the side molding from between the two retainers.
3. Remove the side molding from the vehicle.
4. If the molding is bent or damaged, replace the molding.

### Installation Procedure

1. If the windshield reveal molding retainer clips are bent or damaged, replace the clips.
2. Align the top end of the reveal molding to the end cap tongue inside the opening of the roof rail.
3. Install the reveal molding downward and align the reveal molding with the screw holes.
4. Press down the side molding with even force so as to insert the side molding into the windshield retainer clips.
5. Remove the masking tape.
6. Clean the tape residue from the windshield.