For 1990-2009 cars

## Power Steering Pump Bracket Replacement LH2

### Removal Procedure

1. Remove the power steering pump. Refer to Power Steering Pump Replacement.
2. Remove the power steering pump to bracket bolts.
3. Separate the power steering pump from the power steering bracket.

### Installation Procedure

1. Install the power steering pump to the power steering bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the power steering pump to bracket bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the power steering pump. Refer to Power Steering Pump Replacement.

## Power Steering Pump Bracket Replacement LY7

### Removal Procedure

1. Remove the power steering pump. Refer to Power Steering Pump Replacement.
2. Remove the power steering pump to bracket bolts.
3. Separate the power steering pump from the power steering pump bracket.

### Installation Procedure

1. Install the power steering pump to the power steering bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the power steering pump to power steering pump bracket bolts.

Tighten
Tighten the bolts to 25 N·m (18 lb ft).

3. Install the power steering pump. Refer to Power Steering Pump Replacement .