For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Auxiliary Electric Cooling Fan to Condenser Bolts | 5.4 N·m | 48 lb in
Condenser Bracket Mounting Bolts | 5.4 N·m | 48 lb in
Condenser Mounting Bracket to Radiator Bolts | 5.4 N·m | 48 lb in
Coolant Pipe to Cylinder Head Bolt (LY7) | 50 N·m | 37 lb ft
Coolant Pipe to Thermostat Bolt (LY7) | 10 N·m | 89 lb in
Electric Cooling Fan Blade Nut | 7 N·m | 62 lb in
Electric Cooling Fan Motor Screws | 5 N·m | 44 lb in
Electric Cooling Fan Shroud Bolts | 6.5 N·m | 58 lb in
Engine Control Module (ECM) Nut | 8 N·m | 71 lb in
Evaporative Emission (EVAP) Canister Purge Solenoid Valve Bolt | 12 N·m | 106 lb in
Heater Hose Inlet Fitting | 20 N·m | 15 lb ft
Intake Manifold Clamp | 6 N·m | 53 lb in
Radiator Support Bracket Bolts | 9 N·m | 80 lb in
Radiator Outlet Hose Bracket Bolts | 25 N·m | 18 lb ft
Remote Power Steering Fluid Cooler Pipe to Cooling Fan Shroud Belts | 5.4 N·m | 48 lb in
Surge Tank Bolt | 9 N·m | 80 lb in
Surge Tank Inlet Hose Fitting | 18 N·m | 13 lb ft
Surge Tank Nut | 9 N·m | 80 lb in
Surge Tank Outlet Pipe Bracket Nut | 9 N·m | 80 lb in
Thermostat Bolt (LY7) | 10 N·m | 89 lb in
Thermostat Housing Bolt (LH2) | 10 N·m | 89 lb in
Thermostat Housing Bolt (LY7) | 20 N·m | 15 lb ft
Transmission Oil Cooler (TOC) Bolt | 5 N·m | 44 lb in
Transmission Oil Cooler Line to Cooling Fan Shroud Bolt | 5.4 N·m | 48 lb in
Water Outlet Housing Bolt (LH2) | 25 N·m | 18 lb ft
Water Outlet Housing Bolt (LY7) | 10 N·m | 89 lb in
Water Pump Bolt | 10 N·m | 89 lb in
Water Pump Pulley Bolt | 12 N·m | 106 lb in